|  |  |
| --- | --- |
| 2D Image Sequence (mandatory for all other imaging modalities) | Multiscaler bin width  Image size in pixels  Bidirectional scan  *Optional: Fill fraction*  *Optional: Scan mirror frequency*  *Optional: TAG bits allocation* |
| 3D Volume Sequence | TAG Lens synchronization signal  TAG Lens nominal frequency  Z-axis planes |
| FLIM (can be incorporated with other modalities) | Laser repetition rate |